NBS Specification:



This product is associated with the following NBS Create clause:

35-05-35/135 General fittings, furnishings and equipment system

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[N10 General fixtures/ furnishings/ equipment](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentFactoryBumpRail)

* [350 MISCELLANEOUS FITTINGS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentFactoryBumpRail)

[P20 Unframed isolated trims/ skirtings/ sundry items](https://www.ribaproductselector.com/products/unframed-isolated-trims-skirtings-sundry-items/P20.aspx)

* [170 PROPRIETARY](https://www.ribaproductselector.com/products/proprietary/P20_170.aspx)

Product Specification:

Kent Factory Bump Rail

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Factory Bump Rail

• Type: KFBR-50 /KFBR-75 /KFBRS-50

• Length: 1000 mm /1200 mm /1500 mm /1800 mm

• Material:

- Type: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel

- Thickness: 2 mm /3 mm

- Finish: 320 grit polished and electropolished /Bead blasted /Bead blasted and electropolished /Electropolished /Satin, 320 grit polished /Powder coated

• Configuration:

• Fixing: Bolt-fixed base plate with stainless steel cowl /Hidden sleeve