NBS Specification:



This product is associated with the following NBS Create clause:

35-05-35/135 General fittings, furnishings and equipment system

NBS Specification:



This product is associated with the following NBS clauses:

[N10 General fixtures/ furnishings/ equipment](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentFactoryBumpRail)

* [350 MISCELLANEOUS FITTINGS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentFactoryBumpRail)

[P20 Unframed isolated trims/ skirtings/ sundry items](https://www.ribaproductselector.com/products/unframed-isolated-trims-skirtings-sundry-items/P20.aspx)

* [170 PROPRIETARY](https://www.ribaproductselector.com/products/proprietary/P20_170.aspx)

Product Specification:

Kent Factory Bump Rail

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Factory Bump Rail

 • Type: KFBR-50 /KFBR-75 /KFBRS-50

 • Length: 1000 mm /1200 mm /1500 mm /1800 mm

 • Material:

 - Type: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel

 - Thickness: 2 mm /3 mm

 - Finish: 320 grit polished and electropolished /Bead blasted /Bead blasted and electropolished /Electropolished /Satin, 320 grit polished /Powder coated

 • Configuration:

 • Fixing: Bolt-fixed base plate with stainless steel cowl /Hidden sleeve