NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVCR2654RD)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVCR2654RD)

Product Specification:

KVCR265/4”RD

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Gully

• Type: KVCR265/4” RD /KVCR365/6” RD /KVCR265/4” SQ /KVCR365/6” SQ

• Height: Manufacturer's standard /Bespoke

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

• Flange type: 4” 150lb R/F S/O ANSI Flange /4” PN10 R/F S/O Flange /Damp proof membrane flange /Holding flange /Puddle flange

• Side inlets:

- Type: 1½” BSP nipple /1½” BSP socket /50 mm push fit /Above ground funnel

- Angle: 45° /90° /Bespoke

• Cover/ Grating: Perforated grating /Sealed /Slotted

• Filter basket: Not required /Required /Required, with chain /Required, with separate filter basket

• Accessories: None /Heavy duty suction cup /Hinged self-sealing stainless bung

Suggested Specification:

KVCR265/4”RD

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Gully

• Type: KVCR265/4” RD

• Height: Manufacturer's standard

• Material: 1.4401 (316) stainless steel

• Flange type: Holding flange

• Cover/ Grating: Sealed

• Filter basket: Not required

• Accessories: Heavy duty suction cup