NBS Specification:



This product is associated with the following NBS Create clause:

35-05-35/135 General fittings, furnishings and equipment system

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[N10 General fixtures/ furnishings/ equipment](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentAirportBumpRail)

* [350 MISCELLANEOUS FITTINGS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentAirportBumpRail)

[P20 Unframed isolated trims/ skirtings/ sundry items](https://www.ribaproductselector.com/products/unframed-isolated-trims-skirtings-sundry-items/P20.aspx)

* [170 PROPRIETARY](https://www.ribaproductselector.com/products/proprietary/P20_170.aspx)

Product Specification:

Kent Cleanroom Wall Mounted Bump Rail

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Cleanroom Wall Mounted Bump Rail KCWBR50

• Length: 1250 mm /Bespoke

• Configuration:

• Material:

- Type: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

- Finish: Satin, 320 grit polished

• Fixing: Surface mounted dome nut / Flush countersunk